
PERMIT INSTRUCTIONS PURSUANT TO REGULATIONS

FOR THE CONTROL AND ABATEMENT OF AIR POLLUTION



**COMMONWEALTH OF VIRGINIA**

**DEPARTMENT OF ENVIRONMENTAL QUALITY**

**AIR PERMIT**

**FORM 7 INSTRUCTIONS**

**for**

**NEW SOURCE REVIEW PERMITS**

**and STATE OPERATING PERMITS**



**TABLE OF CONTENTS**

[**General Instructions** 3](#_Toc60731415)

[I. Complete Application 3](#_Toc60731416)

[II. Regional Offices 4](#_Toc60731417)

[A. By County 5](#_Toc60731418)

[B. By City/Locality 6](#_Toc60731419)

[III. Confidential Information 8](#_Toc60731420)

[IV. Toxic Pollutants 10](#_Toc60731421)

[A. State Toxics and Hazardous Air Pollutants (HAPs) 10](#_Toc60731422)

[B. List of Toxics and Federal Hazardous Air Pollutants (HAPs) 11](#_Toc60731423)

[**Instructions for Specific Pages of the Application** 13](#_Toc60731424)

[V. Page 3 - Local Governing Body Certification Form 13](#_Toc60731425)

[VI. Pages 6-8 - Application Fee Form 14](#_Toc60731426)

[A. Instructions 14](#_Toc60731427)

[B. Definitions 14](#_Toc60731428)

[VII. Page 9 - Air Permit Application Checklist 16](#_Toc60731429)

[VIII. Page 10 - Document Certification Form 16](#_Toc60731430)

[IX. Pages 11 and 12 General Information 17](#_Toc60731431)

[X. Page 13 – Fuel Burning Equipment 19](#_Toc60731432)

[XI. Page 14 – Stationary Internal Combustion Engines 19](#_Toc60731433)

[XII. Page 15 – Liquid and/or Solid Waste Incinerators 20](#_Toc60731434)

[XIII. Page 16 – Processing, Manufacturing, Surface Coating & Degreasing Operations 21](#_Toc60731435)

[XIV. Page 17 – Inks, Coatings, Stains, and Adhesives 21](#_Toc60731436)

[XV. Pages 18 and 19 – VOC/Petroleum Liquid Storage Tanks 22](#_Toc60731437)

[XVI. Page 20 – Loading Racks and Oil-Water Separators 23](#_Toc60731438)

[XVII. Page 21 – Fumigation Operations 24](#_Toc60731439)

[XVIII. Page 22 – Air Pollution Control and Monitoring Equipment 24](#_Toc60731440)

[XIX. Page 23 – Air Pollution Control Equipment – Supplemental Information 25](#_Toc60731441)

[XX. Page 24 – Stack Parameters and Fuel Data 26](#_Toc60731442)

[XXI. Page 25 – Proposed Permit Limits for Criteria Pollutants 26](#_Toc60731443)

[XXII. Page 27 – Proposed Permit Limits for Toxic Pollutants/HAPs 27](#_Toc60731444)

[XXIII. Page 26 – Proposed Permit Limits for Other Regulated Pollutants 27](#_Toc60731445)

[XXIV. Page 28 – Proposed Permit Limits for Greenhouse Gases (GHGs) on Mass Basis 28](#_Toc60731446)

[XXV. Page 29 – Proposed Permit Limits for Greenhouse Gases (GHGs) on CO2 Equivalent Emissions (CO2e) Basis 28](#_Toc60731447)

[XXVI. Page 30 – Baseline Actual Emissions (BAE) for Criteria Pollutants 28](#_Toc60731448)

[XXVII. Page 31 – Baseline Actual Emissions (BAE) for Greenhouse Gases (GHGs) Pollutant Emissions on Mass Basis 31](#_Toc60731449)

[XXVIII. Page 32 - Baseline Actual Emissions (BAE) for Greenhouse Gases (GHGs) Pollutant Emissions on CO2 Equivalent Emissions (CO2e) Basis 31](#_Toc60731450)

[XXIX. Page 33 – Operating Periods 32](#_Toc60731451)

# General Instructions

1. **Complete Application**

This is an application form for a new source review permit or a state operating permit. The staff of the Department of Environmental Quality reviews all permit applications to determine compliance with State Regulations. The evaluation of a permit application is a detailed and lengthy process, so your application should be submitted as soon as you can furnish the requisite information**. A complete application is required prior to our commencing the process of preparing a permit. Once you have submitted a complete application, we process your application as quickly as possible**. To expedite the permit application and review process, please supply the information requested on the attached form accurately and completely.

A complete application must include:

|  |  |  |
| --- | --- | --- |
| 1. | ***Form 7*** | A completed Form 7, including a properly signed Document Certification Form. |
| 2. | ***Map\**** | A Source location map that includes latitude and longitude coordinates for the facility. |
| 3. | ***Facility\**** | A site plan of the facility including the dimensions of all buildings (length, width and height), all stack and emission point locations by stack number, and the property lines and fence lines. |
| 4. | ***Process\**** | A process flow diagram/schematic, a narrative process description and a material balance that reflects the requested permit limits. |
| 5. | ***MSDS or CPDS\**** | Material Safety Data Sheets or Certified Product Data Sheets indicating the percent by weight of each ingredient and, for coatings, the VOC content in pounds per gallon. |
| 6. | ***Calculations*** | Calculations of emission estimates. Control technology justification to include economic analysis, if required. |
| 7. | ***Stack Test\**** | Stack test data if applicable. |
| 8. | ***Modeling\**** | Air quality modeling based on consultation with the applicable regional office and the Office of Air Permit Programs, if required. |
| 9. | ***Local Governing\* Body Certification Form*** | Forward the form to local governing body, if applicable. |
| 10. | ***Permit Application Fee Form*** | Include a copy of the Permit Application Fee form with the application, if applicable. |

\*Not required for state operating permit applications unless specifically requested.

INSTRUCTIONS ARE PROVIDED FOR EACH PAGE OF THE FORM 7. Should you require additional assistance in completing this application, please contact the [regional office](https://www.deq.virginia.gov/get-involved/about-us/contact-us) for your area as shown on the map and localities list on pages 4 through 7. Submit the completed application to the appropriate regional office.

***IT IS A VIOLATION OF STATE REGULATIONS TO BEGIN CONSTRUCTION OF OR OPERATE***

***A SOURCE WITHOUT OBTAINING A PERMIT, IF A PERMIT IS REQUIRED***

**\*\*Note:** The Form 7 is available in MS Word on the [DEQ website](https://www.deq.virginia.gov/permits/air/forms). Adobe PDF formats are available upon request.

1. **Regional Offices**



1. **By County**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **County** | **Region** |  | **County** | **Region** |
| Accomack | TRO |  | King and Queen | PRO |
| Albemarle | VRO |  | King George | NRO |
| Alleghany | BRRO |  | King William | PRO |
| Amelia | PRO |  | Lancaster | PRO |
| Amherst | BRRO |  | Lee | SWRO |
| Appomattox | BRRO |  | Loudoun | NRO |
| Arlington | NRO |  | Louisa | NRO |
| Bath | VRO |  | Lunenburg | PRO |
| Bedford | BRRO |  | Madison | NRO |
| Bland | SWRO |  | Mathews | PRO |
| Botetourt | BRRO |  | Mecklenburg | PRO |
| Bristol | SWRO |  | Middlesex | PRO |
| Brunswick | PRO |  | Montgomery | BRRO |
| Buchanan | SWRO |  | Nelson | VRO |
| Buckingham | PRO |  | New Kent | PRO |
| Campbell | BRRO |  | Northampton | TRO |
| Caroline | NRO |  | Northumberland | PRO |
| Carroll | SWRO |  | Norton | SWRO |
| Charles City | PRO |  | Nottoway | PRO |
| Charlotte | BRRO |  | Orange | NRO |
| Chesapeake | TRO |  | Page | VRO |
| Chesterfield | PRO |  | Patrick | BRRO |
| Clarke | VRO |  | Pittsylvania | BRRO |
| Craig | BRRO |  | Powhatan | PRO |
| Culpeper | NRO |  | Prince George | PRO |
| Cumberland | PRO |  | Prince Edward | PRO |
| Dickenson | SWRO |  | Prince William | NRO |
| Dinwiddie | PRO |  | Pulaski | BRRO |
| Essex | PRO |  | Rappahannock | NRO |
| Fairfax | NRO |  | Richmond | PRO |
| Fauquier | NRO |  | Roanoke | BRRO |
| Floyd | BRRO |  | Rockbridge | VRO |
| Fluvanna | VRO |  | Rockingham | VRO |
| Franklin | BRRO |  | Russell | SWRO |
| Frederick | VRO |  | Scott | SWRO |
| Giles | BRRO |  | Shenandoah | VRO |
| Gloucester | PRO |  | Smyth | SWRO |
| Goochland | PRO |  | Southampton | TRO |
| Grayson | SWRO |  | Spotsylvania | NRO |
| Greene | VRO |  | Stafford | NRO |
| Greensville | PRO |  | Surry | PRO |
| Halifax | BRRO |  | Sussex | PRO |
| Hampton | TRO |  | Tazewell | SWRO |
| Hanover | PRO |  | Warren | VRO |
| Henrico | PRO |  | Washington | SWRO |
| Henry | BRRO |  | Westmoreland | PRO |
| Highland | VRO |  | Wise | SWRO |
| Isle of Wight | TRO |  | Wythe | SWRO |
| James City | TRO |  | York | TRO |

|  |  |
| --- | --- |
| [BRRO – Blue Ridge Regional Office](https://www.deq.virginia.gov/get-involved/about-us/contact-us/blue-ridge-regional-office) | [SWRO – Southwest Regional Office](https://www.deq.virginia.gov/get-involved/about-us/contact-us/southwest-regional-office) |
| [NRO – Northern Regional Office](https://www.deq.virginia.gov/get-involved/about-us/contact-us/northern-regional-office) | [TRO – Tidewater Regional Office](https://www.deq.virginia.gov/get-involved/about-us/contact-us/tidewater-regional-office) |
| [PRO – Piedmont Regional Office](https://www.deq.virginia.gov/get-involved/about-us/contact-us/piedmont-regional-office) | [VRO – Valley Regional Office](https://www.deq.virginia.gov/get-involved/about-us/contact-us/valley-regional-office) |

1. **By City/Locality**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **City/Locality** | **Region** |  | **City/Locality** | **Region** |  | **City/Locality** | **Region** |
| Accomac | TRO |  | Chula | PRO |  | Goochland | PRO |
| Achilles | PRO |  | Church View | PRO |  | Gray | PRO |
| Adner | PRO |  | Claremont | PRO |  | Gressitt | PRO |
| Alberta | PRO |  | Clintwood | SWRO |  | Greys Point | PRO |
| Alexandria | NRO |  | Coatesville | PRO |  | Grundy | SWRO |
| Allmondsville | PRO |  | Cobbs Creek | PRO |  | Gum Spring | PRO |
| Amelia Courthouse | PRO |  | Cochran | PRO |  | Gwynn | PRO |
| Ark | PRO |  | Coeburn | SWRO |  | Hadensville | PRO |
| Arlington | NRO |  | Coles Point | PRO |  | Hague | PRO |
| Ashland | PRO |  | Collinsville | BRRO |  | Hallwood | TRO |
| Aylett | PRO |  | Colonial Beach | PRO |  | Hampton | TRO |
| Bacon’s Castle | PRO |  | Colonial Heights | PRO |  | Hanover | PRO |
| Ballsville | PRO |  | Columbia | PRO |  | Harrisonburg | VRO |
| Barhamsville | PRO |  | Covington | BRRO |  | Hartfield | PRO |
| Bavon | PRO |  | Crozier | PRO |  | Haynesville | PRO |
| Beach | PRO |  | Daleville | BRRO |  | Haysi | SWRO |
| Beaverdam | PRO |  | Damascus | SWRO |  | Heathsville | PRO |
| Bedford | BRRO |  | Danieltown | PRO |  | Highland Springs | PRO |
| Belle Haven | TRO |  | Danville | BRRO |  | Hillsville | SWRO |
| Bensley | PRO |  | Darvills | PRO |  | Holdcroft | PRO |
| Bertrand | PRO |  | Deltaville | PRO |  | Hollins | BRRO |
| Big Stone Gap | SWRO |  | Dendron | PRO |  | Homeville | PRO |
| Blacksburg | BRRO |  | DeWitt | PRO |  | Hopewell | PRO |
| Bland | SWRO |  | Dinwiddie | PRO |  | Hull Neck | PRO |
| Bloxom | TRO |  | Disputanta | PRO |  | Independence | SWRO |
| Bon Air | PRO |  | Doswell | PRO |  | Irvington | PRO |
| Boones Mill | BRRO |  | Dublin | BRRO |  | Jarratt | PRO |
| Bottoms Bridge | PRO |  | Dunnsville | PRO |  | Jetersville | PRO |
| Bowlers Wharf | PRO |  | Eagle Rock | BRRO |  | Jonesville | SWRO |
| Brays Fork | PRO |  | Eastville | TRO |  | Keller | TRO |
| Brodnax | PRO |  | Ebony | PRO |  | Kilmarnock | PRO |
| Brunswick | PRO |  | Edgerton | PRO |  | King & Queen | PRO |
| Buchanan | BRRO |  | Elberon | PRO |  | King William | PRO |
| Buena Vista | VRO |  | Emporia | PRO |  | Kinsale | PRO |
| Burgess | PRO |  | Ettrick | PRO |  | Lakeside | PRO |
| Burrowsville | PRO |  | Exmore | TRO |  | Lancaster | PRO |
| Butylo | PRO |  | Fair Port | PRO |  | Lanexa | PRO |
| Cabin Point | PRO |  | Fairfax | NRO |  | Laurel | PRO |
| Callao | PRO |  | Falls Church | NRO |  | Lawrenceville | PRO |
| Cape Charles | TRO |  | Farnham | PRO |  | Lebanon | SWRO |
| Caret | PRO |  | Fife | PRO |  | Leedstown | PRO |
| Carson | PRO |  | Fincastle | BRRO |  | Lerty | PRO |
| Cartersville | PRO |  | Fleeton | PRO |  | Lewisetta | PRO |
| Center Cross | PRO |  | Floyd | BRRO |  | Lexington | VRO |
| Central Garage | PRO |  | Ford | PRO |  | Lilian | PRO |
| Champlain | PRO |  | Franklin | TRO |  | Littleton | PRO |
| Charles City | PRO |  | Fredericksburg | NRO |  | Litwalton | PRO |
| Charlottesville | VRO |  | Galax | SWRO |  | Lively | PRO |
| Cheriton | TRO |  | Gasburg | PRO |  | Loretto | PRO |
| Chesapeake | TRO |  | George’s Tavern | PRO |  | Lottsburg | PRO |
| Chester | PRO |  | Glade Spring | SWRO |  | Low Moor | BRRO |
| Chesterfield | PRO |  | Glen Allen | PRO |  | Lyells | PRO |
| Chilhowie | SWRO |  | Glenns | PRO |  | Lynchburg | BRRO |
| Chincoteague | TRO |  | Gloucester | PRO |  | Maidens | PRO |
| Christiansburg | BRRO |  | Gloucester Point | PRO |  | Manakin-Sabot | PRO |

|  |  |
| --- | --- |
| BRRO – Blue Ridge Regional Office | SWRO – Southwest Regional Office |
| NRO – Northern Regional Office | TRO – Tidewater Regional Office |
| PRO – Piedmont Regional Office | VRO – Valley Regional Office |

**By City/Locality (Continued)**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **City/Locality** | **Region** |  | **City/Locality** | **Region** |  | **City/Locality** | **Region** |
| Manassas | NRO |  | Remlik | PRO |  | Ware Neck | PRO |
| Manassas Park | NRO |  | Richlands | SWRO |  | Wares Wharf | PRO |
| Mangohick | PRO |  | Richmond, City of | PRO |  | Warner | PRO |
| Mannboro | PRO |  | Ridgeway | BRRO |  | Warsaw | PRO |
| Manquin | PRO |  | Ripplemead | BRRO |  | Water View | PRO |
| Marion | SWRO |  | Roanoke | BRRO |  | Waverly | PRO |
| Martinsville | BRRO |  | Rock Castle | PRO |  | Waynesboro | VRO |
| Matoaca | PRO |  | Rockville | PRO |  | Weems | PRO |
| Matthews | PRO |  | Rocky Mount | BRRO |  | West Point | PRO |
| McKenney | PRO |  | Roxbury | PRO |  | White Stone | PRO |
| Meadows of Dan | BRRO |  | Rural Retreat | SWRO |  | White Marsh | PRO |
| Mechanicsville | PRO |  | Saint Stevens Church | PRO |  | White Plains | PRO |
| Melfa | TRO |  | Salem | BRRO |  | Wicomico Church | PRO |
| Midlothian | PRO |  | Saluda | PRO |  | Williamsburg | TRO |
| Millers Tavern | PRO |  | Sandston | PRO |  | Wilsons | PRO |
| Mobjack | PRO |  | Sandy Point | PRO |  | Winchester | VRO |
| Moneta | BRRO |  | Saxis | TRO |  | Windmill Point | PRO |
| Montpelier | PRO |  | Scotland | PRO |  | Winterpock | PRO |
| Montross | PRO |  | Scotts Fork | PRO |  | Wise | SWRO |
| Moon | PRO |  | Severn | PRO |  | Wytheville | SWRO |
| Morattico | PRO |  | Shackelfords | PRO |  | Yale | PRO |
| Morven | PRO |  | Sharps | PRO |  |  |  |
| Moseley | PRO |  | Short Pump | PRO |  |  |  |
| Mount Holly | PRO |  | Skippers | PRO |  |  |  |
| Mundy Point | PRO |  | Smith Point | PRO |  |  |  |
| Narrows | BRRO |  | Spring Grove | PRO |  |  |  |
| Nassawadox | TRO |  | Staunton | VRO |  |  |  |
| Naxera | PRO |  | Stevensville | PRO |  |  |  |
| New Castle | BRRO |  | Stingray Point | PRO |  |  |  |
| New Kent | PRO |  | Stony Creek | PRO |  |  |  |
| New Point | PRO |  | Stratford Hall | PRO |  |  |  |
| Newport | BRRO |  | Stuart | BRRO |  |  |  |
| Newport News | TRO |  | Studley | PRO |  |  |  |
| Newtown | PRO |  | Suffolk | TRO |  |  |  |
| Norfolk | TRO |  | Surry | PRO |  |  |  |
| Nuttsville | PRO |  | Sussex | PRO |  |  |  |
| Oak Grove | PRO |  | Sutherland | PRO |  |  |  |
| Oilville | PRO |  | Tabscott | PRO |  |  |  |
| Old Church | PRO |  | Talleysville | PRO |  |  |  |
| Onancock | TRO |  | Tangier Island | TRO |  |  |  |
| Onley | TRO |  | Tappahannock | PRO |  |  |  |
| Painter | TRO |  | Tazewell | SWRO |  |  |  |
| Parksley | TRO |  | Templeman | PRO |  |  |  |
| Pearisburg | BRRO |  | Trenholm | PRO |  |  |  |
| Petersburg | PRO |  | Troutville | BRRO |  |  |  |
| Poquoson | TRO |  | Urbana | PRO |  |  |  |
| Portsmouth | TRO |  | Valentines | PRO |  |  |  |
| Potomac Beach | PRO |  | Varina | PRO |  |  |  |
| Powhatan | PRO |  | Village | PRO |  |  |  |
| Prince George | PRO |  | Vinton | BRRO |  |  |  |
| Providence Forge | PRO |  | Virginia Beach | TRO |  |  |  |
| Pulaski | BRRO |  | Wachapreague | TRO |  |  |  |
| Purdy | PRO |  | Wakefield | PRO |  |  |  |
| Radford | BRRO |  | Walkerton | PRO |  |  |  |
| Reedville | PRO |  | Walnut Point | PRO |  |  |  |

|  |  |
| --- | --- |
| BRRO – Blue Ridge Regional Office | SWRO – Southwest Regional Office |
| NRO – Northern Regional Office | TRO – Tidewater Regional Office |
| PRO – Piedmont Regional Office | VRO – Valley Regional Office |

1. **Confidential Information**

**\*\*NOTE: If your facility is considering confidential information, please contact your** [**DEQ regional office**](https://www.deq.virginia.gov/get-involved/about-us/contact-us) **and follow the Confidential Guidance Information document at** <https://www.deq.virginia.gov/permits/air/forms> **located under the *Air Permit Application Forms* tab.**

Under the Virginia Freedom of Information Act (FOIA) (*Virginia Code* Title 2.2, Chapter 37) and by regulation ([9VAC5-170-60](https://law.lis.virginia.gov/admincode/title9/agency5/chapter170/section60/)), all information submitted by the applicant is available to anyone requesting the information unless it is certified by the applicant as meeting all of the criteria listed in 9VAC5-170-60 C:

*“In order to be exempt from disclosure to the public under subsection B of this section, the record, report or information must satisfy the following criteria:*

1. *Information for which the company has been taking and will continue to take measures to protect the confidentiality;*
2. *Information that has not been and is not presently reasonably obtainable without the company's consent by private citizens or other firms through legitimate means other than discovery based on a showing of special need in a judicial or quasi-judicial proceeding;*
3. *Information which is not publicly available from sources other than the owner; and*
4. *Information the disclosure of which would cause substantial harm to the owner."*

However, emissions data shall be available to the public without exception (9VAC5-170-60 A). Emissions data include those data meeting the definition found in federal regulations at [40 CFR 2 Sec. 2.301](https://www.ecfr.gov/cgi-bin/text-idx?SID=5bf6ada711b56cbfe915ae02a297dff8&mc=true&node=pt40.1.2&rgn=div5#se40.1.2_1301), which states:

*"Emission data means, with reference to any source of emission of any substance into the air--*

1. *Information necessary to determine the identity, amount, frequency, concentration, or other characteristics (to the extent related to air quality) of any emission which has been emitted by the source (or of any pollutant resulting from any emission by the source), or any combination of the foregoing;*
2. *Information necessary to determine the identity, amount, frequency, concentration, or other characteristics (to the extent related to air quality) of any emission which, under an applicable standard or limitation, the source was authorized to emit (including, to the extent necessary for such purposes, a description of the manner or rate of operation of the source); and*
3. *A general description of the location and/or nature of the source to the extent necessary to identify the source and to distinguish it from other sources (including, to the extent necessary for such purposes, a description of the device, installation, or operation constituting the source)."*

Applicants should consider the "information necessary to determine…" language in the definition, which can include information on throughputs, heat rates, emissions factors, and other characteristics required to derive information on actual or authorized emissions.

In order for DEQ to accept a claim of confidentiality, the applicant must do all of the following:

* Prepare both confidential and non-confidential versions of the application;

*The front page of the confidential copy and any subsequent pages containing confidential information should be labeled or stamped "Confidential," "Proprietary," or "Trade Secret."*

*The public version should indicate which information or data have been removed or blacked out due to confidentiality by labeling those parts or elements of the application as confidential. If an entire page is confidential, there should be a corresponding non-confidential page describing the type of information held confidential, for instance, "Process Flow Diagram (confidential)."*

*The non-confidential version of the application should be structured so that the permit can be written from the information provided in that version. If this is not feasible then the reasons should be documented in the showing provided with the application. DEQ regional offices can provide a copy of the DEQ Air Permitting Confidentiality Policy, which discusses some approaches to structuring applications so that the permit can reflect the non-confidential information.*

* Remove only confidential information

*If a page contains both confidential and non-confidential information, the public version must contain all of the non-confidential information. The applicant may not remove all the information on a page or application section or part because some of the information is confidential.*

* Refrain from confidentiality claims for emission data that cannot be held confidential

*Information necessary to determine emissions or what the source is authorized to emit cannot be held confidential.*

* Prepare and certify a showing document for all information claimed as confidential and has been removed or omitted from the public version of the application.

*The applicant must prepare a document showing that each type of information or data claimed as confidential meets the criteria of 9VAC5-170-60 C as discussed above. The showing document is itself public information subject to FOIA, so the applicant should not include confidential information in the showing document. The applicant must certify the showing.*

*The showing should follow the format of the example provided below. The certification must contain the wording found in the example.*

###### Example Showing

Throughout the referenced application, XYZ Company claims throughputs of Equipment A, B, and C and composition information of our final blended products as confidential.

Throughputs

XYZ protects the confidentiality of this information by:

* Keeping the information under lock and key except when designated employees have need of its use.
* Allowing only those employees who have a “need to know” access to this information. Other XYZ employees do not have access to this information.
* Requiring all employees who have access to this information to sign a confidentiality agreement.

Disclosure of the throughputs of Equipment A, B, and C could cause substantial harm to XYZ by allowing competitors to better determine our costs. Both fixed and variable costs in our industry are highly dependent on the scale of operations. Disclosure of this information would give competitors information with which they could determine our production capacity, which we believe they do not know at this time. To the best of our knowledge, this information is not publicly available and is not reasonably obtainable by the public or other unauthorized parties.

Product Composition

XYZ protects the confidentiality of this information by:

* Keeping the information under lock and key except when designated employees have need of its use.
* Allowing only those employees who have a “need to know” access to this information. Other XYZ employees do not have access to this information.
* Requiring all employees who have access to this information to sign a confidentiality agreement.
* Requiring customers who have access to this information to sign confidentiality agreements

Disclosure of the composition of our final blended products could cause substantial harm to XYZ by allowing competitors to reverse engineer our products. XYZ has invested significant resources over many years developing these products. Disclosure of these compositions could allow competitors to copy our products without them being required to expend the resources we have spent developing them, thereby reducing our current competitive advantage. To the best of our knowledge, this information is not publicly available and is not reasonably obtainable by the public or other unauthorized parties.

Certification

I hereby certify under penalty of law that to the best of my knowledge and belief, after diligent inquiry, the information claimed above as confidential meets the confidential information criteria of 9VAC5-170-60 C and 40 CFR 2.208 and is not "emissions data." Further, to the best of my knowledge, this information has never been determined not to be confidential information by EPA or any other agency, nor has it ever been disclosed to the public by EPA or any other agency.

Typed Name and Title of Responsible Official \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature of Responsible Official \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

DEQ staff will review the material to determine its eligibility for confidential treatment and will inform you in writing of the determination.

1. **Toxic Pollutants**
2. **State Toxics and Hazardous Air Pollutants (HAPs)**

Proposed projects that emit one or more state toxic air pollutants are evaluated under [9VAC5 Chapter 80, Article 5](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section800/) of the Commonwealth of Virginia State Air Pollution Control Board Regulations for the Control and Abatement of Air Pollution (Regulation). The list of state toxics can be found on the following page. Unless exempt under [9VAC5-60-300 C](https://law.lis.virginia.gov/admincode/title9/agency5/chapter60/section300/)., proposed projects with toxics emissions above the corresponding calculated hourly and/or annual exemption threshold levels must apply Best Available Control Technology (BACT) to minimize air toxic emissions. Since many of the air toxics are also either volatile organic compounds (VOC) or particulate matter compounds, control measures that reduce these criteria pollutant emissions may be used to reduce air toxic emissions. In addition, the applicant must demonstrate through air dispersion modeling that the concentration of the air toxic does not exceed the corresponding Significant Ambient Air Concentration (SAAC). The SAAC is the concentration of a toxic pollutant in the ambient air that, if exceeded, may have an adverse effect to human health.

Exemption and SAAC values for each air toxic can be found at the following link: [Calculated exemption levels and SAACs for each Air Toxic Pollutant](https://www.deq.virginia.gov/home/showpublisheddocument?id=5546)

Proposed projects with federal hazardous air pollutant emissions ([HAPs](https://www.epa.gov/haps/initial-list-hazardous-air-pollutants-modifications)) are evaluated for National Emission Standards for Hazardous Air Pollutant (NESHAP) (commonly referred to as maximum achievable control technology or MACT) applicability and to establish whether or not the proposed project will be a major or area source of HAPs. A major source of HAPs means any stationary source or group of stationary sources located within a contiguous area and under common control that emits or has the potential to emit 10 tons per year or more of any individual HAP or 25 tons per year or more of any combination of HAPs. An area source is one that is not major.

New or modified projects that are a major source of HAPs and are not subject to a promulgated NESHAP are subject to permitting under [9VAC5 Chapter 80, Article 7](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1400/) of the Regulation.

If a proposed project includes some units that are covered by a NESHAP and some that are not, the units not covered by the NESHAP need to be evaluated under the state toxics regulation.

For further details, please contact the appropriate [DEQ regional office](https://www.deq.virginia.gov/get-involved/about-us/contact-us) and/or check out [air Toxics Information](https://www.deq.virginia.gov/permits-regulations/permits/air) on the DEQ website.

1. **List of Toxics and Federal Hazardous Air Pollutants (HAPs)**

| **DEPARTMENT OF ENVIRONMENTAL QUALITY**  **HAZARDOUS AIR POLLUTANT LIST** PAGE 1 OF 2 | |
| --- | --- |
| CAS# NAME  75‑07‑0 ACETALDEHYDE  60‑35‑5 ACETAMIDE  75‑05‑8 ACETONITRILE  98‑86‑2 ACETOPHENONE  53‑96‑3 2‑ACETYLAMINOFLUORENE  107‑02‑8 ACROLEIN  79‑06‑1 ACRYLAMIDE  79‑10‑7 ACRYLIC ACID  107‑13‑1 ACRYLONITRILE  107‑05‑1 ALLYL CHLORIDE  92‑67‑1 4‑AMINODIPHENYL  62‑53‑3 ANILINE & HOMOLOGUES  90-04-0 o-ANISIDINE  ----------- ANTIMONY COMPOUNDS1  ----------- ARSENIC COMPOUNDS  71‑43‑2 BENZENE (including benzene from gasoline)  92‑87‑5 BENZIDINE  98‑07‑7 BENZOTRICHLORIDE  100‑44‑7 BENZYL CHLORIDE  ----------- BERYLLIUM COMPOUNDS  92‑52‑4 BIPHENYL  72‑55‑9 2,2‑BIS(p‑CHLORPHENYL)‑1,1‑DICHLORO- ETHYLENE/DDE  75‑25‑2 BROMOFORM   * 1. 1,3-BUTADIENE   ----------- CADMIUM COMPOUNDS  156‑62‑7 CALCIUM CYANAMIDE  133‑06‑2 CAPTAN  63‑25‑2 CARBARYL  75‑15‑0 CARBON DISULFIDE  56‑23‑5 CARBON TETRACHLORIDE  463‑58‑1 CARBONYL SULFIDE  120‑80‑9 CATECHOL  79‑11‑8 CHLOROACETIC ACID  133‑90‑4 CHLORAMBEN  57‑74‑9 CHLORDANE  7782‑50‑5 CHLORINE  126‑99‑8 ß-CHLOROPRENE / 2‑CHLORO‑1,3‑BUTADIENE  532‑27‑4 2‑CHLOROACETOPHENONE  108‑90‑7 CHLOROBENZENE  510‑15‑6 CHLOROBENZILATE  67‑66‑3 CHLOROFORM  107‑30‑2 CHLOROMETHYL METHYL ETHER / CMME  542‑88‑1 BIS-(CHLOROMETHYL) ETHER  ----------- CHROMIUM COMPOUNDS  ----------- COBALT COMPOUNDS  ----------- COKE OVEN EMISSIONS  1319‑77‑3 CRESOLS / CRESYLIC ACID  95-48-7 o-CRESOL  108-39-4 m-CRESOL  106-44-5 P-CRESOL  98‑82‑8 CUMENE  ----------- CYANIDE COMPOUNDS2  94‑75‑7 2,4‑DICHLOROPHENOXYACETIC ACID (including salts and esters)  117‑81‑7 DI‑SEC‑OCTYL PHTHALATE / BIS(2- ETHYLHEXYL)PHTHALATE  334‑88‑3 DIAZOMETHANE | CAS# NAME  132-64-9 DIBENZOFURANS  96‑12‑8 1,2‑DIBROMO‑3‑CHLOROPROPANE  84‑74‑2 DIBUTYL PHTHALATE  106‑46‑7 1-4 DICHLOROBENZENE  91‑94‑1 3,3'‑DICHLOROBENZIDENE  75‑34‑3 1,1‑DICHLOROETHANE / ETHYLIDENE  DICHLORIDE  107‑06‑2 1,2‑DICHLOROETHANE / ETHYLENE  DICHLORIDE  111‑44‑4 DICHLOROETHYL ETHER /  BIS(2-CHLOROETHYL)ETHER  542‑75‑6 1,3‑DICHLOROPROPENE  62‑73‑7 DICHLORVOS  111‑42‑2 DIETHANOLAMINE  64‑67‑5 DIETHYL SULFATE  119‑90‑4 3,3‑DIMETHOXYBENZIDINE  60‑11‑7 DIMETHYL AMINOAZOBENZENE /  4-DIMETHYLAMINOAZOBENZENE  79‑44‑7 DIMETHYL CARBAMOYL CHLORIDE  77‑78‑1 DIMETHYL SULFATE  121‑69‑7 DIMETHYLANILINE  119‑93‑7 3,3‑DIMETHYLBENZIDINE  68‑12‑2 DIMETHYL FORMAMIDE / N,N-  DIMETHYLFORMAMIDE  57‑14‑7 1,1‑DIMETHYLHYDRAZINE  131‑11‑3 DIMETHYL PHTHALATE  534‑52‑1 4,6‑DINITRO‑o‑CRESOL (including Salts)  51‑28‑5 2,4‑DINITROPHENOL  121‑14‑2 2,4‑DINITROTOLUENE  123‑91‑1 1,4‑DIOXANE / 1,4-DIETHYLENEOXIDE  122‑66‑7 1,2‑DIPHENYLHYDRAZINE  106‑89‑8 EPICHLOROHYDRIN  106‑88‑7 1,2‑EPOXYBUTANE  110-80-5 2-ETHOXYETHANOL 3  140‑88‑5 ETHYL ACRYLATE  100‑41‑4 ETHYL BENZENE  51‑79‑6 ETHYL CARBAMATE / URETHANE   * + 1. ETHYL CHLORIDE / CHLOROETHANE   106‑93‑4 ETHYLENE DIBROMIDE / EDB / 1,2-  DIBROMOETHANE  107‑21‑1 ETHYLENE GLYCOL  75‑21‑8 ETHYLENE OXIDE  96‑45‑7 ETHYLENE THIOUREA / ETU  151‑56‑4 ETHYLENIMINE  50‑00‑0 FORMALDEHYDE  ----------- GLYCOL ETHERS3  76‑44‑8 HEPTACHLOR  118‑74‑1 HEXACHLOROBENZENE  87‑68‑3 HEXACHLOROBUTADIENE  The following pollutants and pollutant source categories are listed as HAPs under section 112(b) but are excluded from the definitions of toxics in the Virginia Regulations:     1. Asbestos NESHAP, 40 CFR 61 Subpart M (for asbestos removal, demolition and installation contact Virginia Department of Labor - 804/786-8009).   2. Fine Mineral Fibers.  3. Radionuclides (including radon). |

| **DEPARTMENT OF ENVIRONMENTAL QUALITY**  **HAZARDOUS AIR POLLUTANT LIST** PAGE 2 OF 2 | |
| --- | --- |
| CAS# NAME  77‑47‑4 HEXACHLOROCYCLOPENTADIENE  67‑72‑1 HEXACHLOROETHANE  680‑31‑9 HEXAMETHYL PHOSPHORAMIDE / HMPA  822‑06‑0 HEXAMETHYLENE DIISOCYANATE  110‑54‑3 HEXANE  302‑01‑2 HYDRAZINE  7647‑01‑0 HYDROGEN CHLORIDE/ HYDROCHLORIC  ACID (gas only)  7664‑39‑3 HYDROGEN FLUORIDE / HYDROFLUORIC ACID  123‑31‑9 HYDROQUINONE / DIHYDROXYBENZENE  78‑59‑1 ISOPHORONE  109-59-1 ISOPROPOXYETHANOL 3  ----------- LEAD COMPOUNDS  58-89-9 LINDANE (AND ALL OTHER STEREOISOMERS OF  1,2,3,4,5,6-HEXACHLOROCYCLOHEXANE )  108‑31‑6 MALEIC ANHYDRIDE  ----------- MANGANESE COMPOUNDS  ----------- MERCURY COMPOUNDS  67‑56‑1 METHANOL  72‑43‑5 METHOXYCHLOR  109-86-4 2-METHOXYETHANOL 3  74‑83‑9 METHYL BROMIDE / BROMOMETHANE  74‑87‑3 METHYL CHLORIDE / CHLOROMETHANE  71‑55‑6 METHYL CHLOROFORM / 1,1,1-  TRICHLOROETHANE  60‑34‑4 METHYL HYDRAZINE  74‑88‑4 METHYL IODIDE/IODOMETHANE  108‑10‑1 METHYL ISOBUTYL KETONE / HEXONE  624‑83‑9 METHYL ISOCYANATE  80‑62‑6 METHYL METHACRYLATE  1634‑04‑4 METHYL TERT BUTYL ETHER  101‑14‑4 4,4- METHYLENE BIS(2‑CHLOROANILINE)  101‑68‑8 4,4'-METHYLENE DIPHENYL DIISOCYANATE /  MDI  75‑09‑2 METHYLENE CHLORIDE / DICHLOROMETHANE  101‑77‑9 4,4-METHYLENE DIANILINE  91‑20‑3 NAPHTHALENE  ----------- NICKEL COMPOUNDS  98‑95‑3 NITROBENZENE  92‑93‑3 4‑NITROBIPHENYL  100‑02‑7 4‑NITROPHENOL  79‑46‑9 2‑NITROPROPANE  684‑93‑5 N‑NITROSO‑N‑METHYLUREA / NMU  62‑75‑9 N‑NITROSODIMETHYLAMINE / NDMA  59‑89‑2 N‑NITROSOMORPHOLINE / NMOR  56‑38‑2 PARATHION  82‑68‑8 PENTACHLORONITROBENZENE /  QUINTOBENZENE  87‑86‑5 PENTACHLOROPHENOL  108‑95‑2 PHENOL  106‑50‑3 P‑PHENYLENEDIAMINE  75‑44‑5 PHOSGENE / CARBONYLCHLORIDE  7803‑51‑2 PHOSPHINE  7723‑14‑0 PHOSPHORUS  85‑44‑9 PHTHALIC ANHYDRIDE  1336‑36‑3 POLYCHLORINATED BIPHENYLS /  AROCHLORS  ----------- POLYCYCLIC ORGANIC MATTER / POM4  1120‑71‑4 1,3‑PROPANE SULTONE  57‑57‑8 ß‑PROPIOLACTONE  123‑38‑6 PROPIONALDEHYDE  114‑26‑1 PROPOXUR / BAYGON  78‑87‑5 PROPYLENE DICHLORIDE / 1,2-  DICHLOROPROPANE  75‑55‑8 1,2‑PROPYLENE IMINE | CAS# NAME  75‑56‑9 PROPYLENE OXIDE / 1,2-EPOXYPROPANE  91‑22‑5 QUINOLINE  106‑51‑4 QUINONE  ----------- SELENIUM COMPOUNDS  100‑42‑5 STYRENE, MONOMER / VINYL BENZENE  96‑09‑3 STYRENE OXIDE  1746‑01‑6 2,3,7,8‑TETRACHLORODIBENZO‑p‑DIOXIN  79‑34‑5 1,1,2,2‑TETRACHLOROETHANE  127‑18‑4 TETRACHLOROETHYLENE /  PERCHLOROETHYLENE  7550‑45‑0 TITANIUM TETRACHLORIDE  108‑88‑3 TOLUENE  95‑80‑7 2,4‑TOLUENE DIAMINE / TOLUENE‑2,4‑DIAMINE  584‑84‑9 TOLUENE‑2,4‑DIISOCYANATE / TDI  95‑53‑4 O‑TOLUIDINE  8001‑35‑2 TOXAPHENE / CHLORINATED CAMPHENE  120‑82‑1 1,2,4‑TRICHLOROBENZENE  79‑00‑5 1,1,2‑TRICHLOROETHANE  79‑01‑6 TRICHLOROETHYLENE  95‑95‑4 2,4,5‑TRICHLOROPHENOL  88‑06‑2 2,4,6‑TRICHLOROPHENOL  121‑44‑8 TRIETHYLAMINE  1582‑09‑8 TRIFLURALIN  540‑84‑1 2,2,4‑TRIMETHYLPENTANE  108‑05‑4 VINYL ACETATE  593‑60‑2 VINYL BROMIDE  75‑01‑4 VINYL CHLORIDE / CHLOROETHYLENE  75‑35‑4 VINYLIDENE CHLORIDE / 1,1-  DICHLOROETHYLENE  1330-20-7 XYLENE ISOMERS AND MIXTURES  95-47-6 O-XYLENE  108-38-3 M-XYLENE   * + 1. P-XYLENE   1For all listing above which contain the word "compounds" and for glycol ethers, the following applies: Unless otherwise specified, these listings are defined as including any unique chemical substance that contains the named chemical as part of that chemical's infrastructure.  2X'CN where X=H' or any other group where a formal dissociation may occur. For example, KCN or Ca(CN)2  3Glycol ethers include mono- and di-ethers of ethylene glycol, diethylene glycol, and triethylene glycol R-(OCH2CH2)n-OR'  where: n = 1, 2, or 3  R = alkyl C7 or less, or phenyl or alkyl substituted phenyl  R' = H, or alkyl C7 or less, or carboxylic acid ester, sulfate, phosphate, nitrate, or sulfonate  2-Ethoxyethanol, Isopropoxyethanol, and 2-Methoxyethanol meet this definition, but are considered as only one HAP (glycol ethers) for Title V and CAAA §112 purposes. They are also listed individually in this table as a reminder that because they have TLVs, they must be considered separately under Virginia's Toxic Pollutant regulations (9VAC5 Chapter 60, Articles 4 and 5).  4Includes substituted and/or unsubstituted polycyclic aromatic hydrocarbons and aromatic heterocycle compounds, with two or more fused rings, at least one of which is benzenoid in structure. Polycyclic Organic Matter is a mixture of organic compounds containing one or more of these polycyclic aromatic chemicals which include dioxins and furans. Polycyclic Organic Matter is generally formed or emitted during thermal processes including (1) incomplete combustion, (2) pyrolysis, (3) the volatilization, distillation or processing of fossil fuels or bitumens, or (4) the distillation or thermal processing of non-fossil fuels. |

# Instructions for Specific Pages of the Application

1. **Page 3 - Local Governing Body Certification Form**

Effective July 1, 1993, Section 10.1-1321.1 of the Code of Virginia specifies that:

***"A. No application for a permit for a new or major modified stationary air pollution source shall be considered complete unless the applicant has provided the Director with notification from the governing body of the county, city, or town in which the source is to be located that the location and operation of the source are consistent with all ordinances adopted pursuant to Chapter 22 (15.2-2200 et seq.) of Title 15.2."***

"B. The governing body shall inform in writing the applicant and the Department of the source's compliance or noncompliance not more than 45 days from receipt by the chief executive officer, or his agent, of a request from the applicant."

"C. Should the governing body fail to provide written notification as specified in subsection B of this section, the requirement for such notification as specified in subsection A of this section is waived."

Definitions:

* Any new site (not previously designated as a stationary source) upon which one or more emissions units undergo initial construction, installation, or relocation shall be considered a **New Source**.
* Any existing stationary source making changes to emission units (construction, installation, modification, reconstruction, or relocation) shall be considered a **Modified Source**. Modified sources need only use this form if the modification is major.
* Any stationary source that emits, or has the potential to emit, 100 tons or more per year of any regulated air pollutant shall be considered a “**Major Source**”. “Regulated air pollutant” is defined in [9VAC5-80-1110 C](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1110/).
* Any modified source, the modification of which is equivalent to the definition of a "major source", shall be considered a **Major Modified Source**.
* Any “major source”, the modification of which results in a “significant” net emissions increase of any regulated pollutant, shall be considered a **Major Modified Source**.
* Emissions levels that are considered **Significant** for stationary sources located in Prevention of Significant Deterioration Areas are listed in the definition of “significant” in [9VAC5-80-1615 C](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1615/). Emission levels that are considered “significant” for stationary sources located in Non-attainment Areas are listed in the definition of “significant” in [9VAC5-80-2010 C](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section2010/).

If required, the attached form should be submitted for all applications to the appropriate officials of the county, city, or town in which your facility is to be located. (The form is not required for Operating Permits insofar as these pertain to previously existing and operating sources.)

1. **Applicant:** Fill out the top section of the form and sign in the center block. Send the partially completed notification form to the local governing body by certified mail/return receipt, and keep a copy of the return receipt. A copy of the return receipt should then be submitted with the application to the appropriate [DEQ regional office](https://www.deq.virginia.gov/get-involved/about-deq/contact-us).

2. **Local officials**: You may use either this form or a certification designed by the locality. If you use this form, please fill out the bottom section of the form. The form asks you to certify that the facility is or will be consistent with all applicable local ordinances. Please check the appropriate box, sign the form and if there is inconsistency, please attach an explanation that indicates the corrective measures being taken. Then forward the form (or the certification designed by the locality) to the appropriate [DEQ regional office](https://www.deq.virginia.gov/get-involved/about-us/contact-us) within 45 days following receipt of the request from the applicant. (A postmark date within 45 days of receipt is sufficient.) Send a copy of the completed form to the applicant.

There are two ways for an applicant for a new or major modified stationary air pollution source permit to comply with this requirement. (1) When a completed form is received by DEQ indicating that locality certifies that the location and operation of the proposed source are in compliance with local ordinances, then this requirement is met. (2) If the locality fails to respond in writing to the request within 45 days of receipt, then this requirement is met when the applicant provides DEQ with evidence that the locality has received the form and has failed to respond in writing within the 45-day period.

1. **Pages 6-8 - Application Fee Form**
2. **Instructions**

As of July 1, 2012, air permit applications are subject to a fee. See the DEQ website for the most recent [air permitting fee information](https://www.deq.virginia.gov/laws-regulations/air/fees-under-the-air-pollution-control-law). **Fees do not apply to administrative amendments or** true minor sources. Applications will be considered incomplete if the proper fee is not paid and will not be processed until full payment is received. **Air permit application fees are not refundable.**

**Fees are adjusted January 1 of each calendar year.**

**Step 1:** Send the **ORIGINAL** feeform and a check (or money order) payable to “Treasurer of Virginia” to:

**Department of Environmental Quality Department of Environmental Quality**

**Receipts Control OR** **Receipts Control**

**P.O. Box 1104 FOR OVERNIGHT 1111 East Main Street, Suite 1400**

**Richmond, VA 23218 DELIVERY Richmond, VA 23219**

**Step 2:** Send a **COPY** of the fee form with the permit application to the appropriate[**DEQ Regional Office**](https://www.deq.virginia.gov/get-involved/about-us/contact-us)

**Step 3:** Retain a copy for your records. Questions should be directed to the DEQ regional office where the application will be submitted

1. **Definitions**

***Administrative amendment***– An administrative change to a permit issued pursuant to Article 1 (9VAC5-80-50 et seq.), Article 3 (9VAC5-80-360 et seq.), Article 5 (9VAC5-80-800 et seq.), Article 6 (9VAC5-80-1100 et seq.), Article 7 (9VAC5-80-1400 et seq.), Article 8 (9VAC5-80-1605 et seq.), or Article 9 (9VAC5-80-2000 et seq.) of 9VAC5 Chapter 80. Administrative amendments include, but are not limited to, the following:

* corrections of typographical or any other error, defect or irregularity which does not substantially affect the permit,
* identification of a change in the name, address, or phone number of any person identified in the permit, or of a similar minor administrative change at the source,
* change in ownership or operational control of a source where the board determines that no other change in the permit is necessary, provided that a written agreement containing a specific date for transfer of permit responsibility, coverage, and liability between the current and new permittee has been submitted to the board

***Major new source review permit (Major NSR permit****)* – A permit issued pursuant to Article 7 (9VAC5-80-1400 et seq.), Article 8 (9VAC5-80-1605 et seq.), or Article 9 (9VAC5-80-2000 et seq.) of 9VAC5 Chapter 80**. For purposes of fees, the Major NSR permit also includes applications for projects that are major modifications**.

* An Article 7 permit is a preconstruction review permit (case-by-case Maximum Achievable Control Technology (MACT) determination) for the construction or reconstruction of any stationary source or emission unit that has the potential to emit, considering controls, 10 tons per year or more of any individual hazardous air pollutant (HAP) or 25 tons per year or more of any combination of HAPs and EPA has not promulgated a MACT standard or delisted the source category.
* An Article 8 permit is for a source (1) with the potential to emit over 250 tons per year of a single criteria pollutant OR (2) is in one of the listed source categories under [9VAC5-80-1615](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1615/) and has the potential to emit over 100 tons per year of any criteria pollutant OR (3) with the potential to emit over 100,000 tons per year of CO2 equivalent (CO2e) (9VAC5-85 Part IIl). PSD permits are issued in areas that are in attainment of the National Ambient Air Quality Standards.
* An Article 9 permit is a preconstruction review permit for areas that are in nonattainment with a National Ambient Air Quality Standard (NAAQS). Nonattainment permits are required by any major new source that is being constructed in a nonattainment area and is major for the pollutant for which the area is in nonattainment. Nonattainment permitting requirements may also be triggered if an existing minor source makes a modification that results in the facility being major for the pollutant for which the area is in nonattainment. A major source is any source with potential to emit over 250 tons per year of a single criteria pollutant or is in one of the listed source categories under [9VAC5-80-2010](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section2010/) and the potential to emit over 100 tons per year of any criteria pollutant. However, if any area is in nonattainment for a specific pollutant, the major source threshold may be

lower for that pollutant. For example, sources locating in the Northern Virginia Ozone Nonattainment Area which are part of the [Ozone Transport Region](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section2010/) would be a major source if they have the potential to emit more than 100 tons per year of NOX and/or 50 tons per year of VOC regardless of source category. Nonattainment permits do not require an air quality analysis but require a source to control to the Lowest Achievable Emission Rate (LAER) and to obtain offsets.

***Major NSR permit amendment*** – A change to a permit issued pursuant to Article 7 (9VAC5-80-1400 et seq.), Article 8 (9VAC5-80-1605 et seq.), or Article 9 (9VAC5-80-2000 et seq.) of 9VAC5 Chapter 80. **Only minor amendments and significant amendments are included in this category.**

***Minor new source review permit (Minor NSR permit)***– A permit to construct and operate issued under Article 6 (9VAC5-80-1100 et seq.) of 9VAC5 Chapter 80. Minor NSR permits are 1) categorically required; or 2) issued to sources whose uncontrolled emission rate for a regulated criteria pollutant is above exemption thresholds and permitting allowables are below Title V thresholds, and/or 3) issued to sources whose potential to emit for a toxic pollutant is above state toxic exemption thresholds and permitting allowables are below Title V thresholds. The minor NSR permit can be used to establish synthetic minor limits for avoidance of state major, PSD and/or Title V permits. **For purposes of fees, the Minor NSR permit also includes exemption applications and applications for projects at existing sources.**

***Minor NSR amendment*** - A change to a permit issued pursuant to Article 6 (9VAC5-80-1100 et seq.) of 9VAC5 Chapter 80. **Only minor amendments and significant amendments are included in this category.**

***Sources subject to Synthetic Minor permitting requirements*** *-* Stationary sources whose potential to emit exceeds the Title V threshold (100 tons per year of a criteria pollutant and/or 10/25 tpy of HAPs) but have taken federally enforceable limits, either through a state operating permit or a minor NSR permit, to avoid Title V permit applicability.

***Sources subject to Title V permitting requirements*** *–* Stationary sources that have a potential to emit above the Title V thresholds or are otherwise applicable to the Title V permitting program.

***State major permit*** – A permit to construct and operate issued under Article 6 (9VAC5-80-1100 et seq.) of 9VAC5 Chapter 80. State major permits are for facilities that have an allowable emission rate of more than 100 tons per year, but less than 250 tons per year, of any criteria pollutant and are not listed in the 28 categories under “major stationary source” as defined in [9VAC5-80-1615](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1615/).

***State operating permit (SOP****)* – A permit issued under Article 5 (9VAC5-80-800 et seq.) of 9VAC5 Chapter 80. SOPs are most often used by stationary sources to establish federally enforceable limits on potential to emit to avoid major New Source Review permitting (PSD and Nonattainment permits), Title V permitting, and/or major source MACT applicability. SOPs can also be used to combine multiple permits from a stationary source into one permit or to implement emissions trading requirements. The State Air Pollution Control Board, at its discretion, may also issue SOPs to cap the emissions of a stationary source or emissions unit causing or contributing to a violation of any air quality standard or to establish a source-specific emission standard or other requirement necessary to implement the federal Clean Air Act or the Virginia Air Pollution Control Law.

***SOP permit amendment*** - A change to a permit issued pursuant to Article 5 (9VAC5-80-800 et seq.) of 9VAC5 Chapter 80. **Only minor amendments and significant amendments are included in this category.**

***Title V permit*** – A federal operating permit issued pursuant to Article 1 (9VAC5-80-50 et seq.) or Article 3 (9VAC5-80-360 et seq.) of 9VAC5 Chapter 80. Facilities which (1) have the potential to emit of air pollutants above the major source thresholds, listed in [9VAC5-80-60](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section60/) OR (2) are area sources of hazardous air pollutants, not explicitly exempted by EPA. (9VAC5-85 Part IIl), are required to obtain a Title V permit. For purposes of fees, the Title V permit also includes Acid Rain (Article 3) permit applications.

***Title V permit modification*** - A change to a permit issued pursuant to Article 1 (9VAC5-80-50 et seq.) or Article 3 (9VAC5-80-360 et seq.) of 9VAC5 Chapter 80. Only minor modifications and significant modifications are included in this category.

***Title V permit renewal*** – A renewal of a Title V permit pursuant to Article 1 (9VAC5-80-50 et seq.) of 9VAC5 Chapter 80. Title V permits are renewed every 5 years and a renewal application must be submitted to the regional office no sooner than 18 months and no later than 6 months prior to expiration of the current Title V permit. For purposes of fees, the Title V permit renewal also includes Acid Rain (Article 3) permit renewal applications.

***True minor source*** – A source that does not have the physical or operational capacity to emit major amounts (even if the source owner and regulatory agency disregard any enforceable limits). Additional information is available on the [DEQ website](https://www.deq.virginia.gov/permits/air).

1. **Page 9 - Air Permit Application Checklist**

Use the Air Permit Application Checklist page to “√” which application pages are included with the air permit application submission as well as the number of page copies provided.

Also “√” and list attachments included with the air permit application submission as well as the number of copies provided.

1. **Page 10 - Document Certification Form**

Various provisions of the Regulations for the Control and Abatement of Air Pollution require that certain documents submitted to the Board or the Department be signed by a responsible official with certification that the information contained in the statement is accurate to the best knowledge of the individual certifying the statement. Documents covered by this requirement include, but are not limited to, permit applications, registrations, emission statements, emission testing and monitoring reports, or compliance certifications. The certification should include the full name, title, signature, date of signature, and telephone number of the responsible official. A responsible official is defined as follows ([9VAC5-20-230 A](https://law.lis.virginia.gov/admincode/title9/agency5/chapter20/section230/).):

1. For a business entity, such as a corporation, association or cooperative, a responsible official is either:
2. The president, secretary, treasurer, or a vice-president of the business entity in charge of a principal business function, or any other person who performs similar policy or decision-making functions for the business entity; or
3. A duly authorized representative of such business entity if the representative is responsible for the overall operation of one or more manufacturing, production, or operating facilities applying for or subject to a permit and either (i) the facilities employ more than 250 persons or have gross annual sales or expenditures exceeding $25 million (in second quarter 1980 dollars), or (ii) the authority to sign documents has been assigned or delegated to such representative in accordance with procedures of the business entity.
4. For a partnership or sole proprietorship, a responsible official is a general partner or the proprietor, respectively.
5. For a municipality, state, federal, or other public agency, a responsible official is either a principal executive officer or ranking elected official. A principal executive officer of a federal agency includes the chief executive officer having responsibility for the overall operations of a principal geographic unit of the agency.

**Certification is required with each application submittal, including amendments to an application (e.g., new pages, revisions to existing pages and other amendments to application information).**

Reference: Regulations, [9VAC5-80-1140 D](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1140/). Letters, phone calls, etc. are considered additional supplementary information to the certified application submittal.

1. **Pages 11 and 12 General Information**

**PERSON COMPLETING FORM AND DATE –** Provide the name of the person that completed the form, along with the date completed.

**REGISTRATION NUMBER** **–** Give the registration number assigned to the facility if applicable.

**COMPANY AND DIVISION NAME** **–** List the official company name and the division if applicable.

**FIN –** Give the federal ID number assigned to the facility.

**MAILING ADDRESS** **–** List the mailing address that corresponds to the facility on this application.

**EXACT SOURCE LOCATION** **–** Provide a description of the facility location indicating street address (911 address if available) or directions to facility; provide a map pinpointing the exact source location and specify where the plant property boundaries are, if requested by the regional office; provide a plant layout with dimensions of all buildings (height, length, width) at the facility indicating all stack and emission point locations by stack or reference number, if requested.

**FACILITY PHONE NUMBER** **–** List the phone number at the facility.

**NUMBER OF EMPLOYEES AT SITE** **–** List the number of employees at the facility.

**PROPERTY AREA AT SITE** **–** List the area in acres.

**PERSON TO CONTACT ON AIR POLLUTION MATTERS** **–** Provide the name/title of a contact person for air pollution matters.

**CONTACT PHONE NUMBER** **–** Provide a phone number at which DEQ staff can reach the contact person.

**CONTACT E-MAIL ADDRESS** **–** Provide an E-mail address of the contact person.

**CONTACT FAX NUMBER** **–** Provide the fax number of the contact person, if there is one.

**LAT/LONG COORDINATES OR UTM COORDINATES OF FACILITY** – Provide the latitude and longitude coordinates or UTM Coordinates of the facility.

**REASON(S) FOR SUBMISSION** **–** Check the appropriate box(es) and the applicable regulation(s).

1. "STATE OPERATING PERMIT" means that you are either an existing source applying for an operating permit or are a NEW SOURCE applying for a State Operating Permit concurrently with a permit to construct and operate the NEW SOURCE. State Operating Permits are normally optional, and are requested for one of the reasons stated in [9VAC5-80-800 C](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section800/).
2. "NEW SOURCE" means that you are either constructing emission units at a new facility where no facility now exists, or you are constructing emission units at a facility that previously had no emission units at the facility. The NEW SOURCE is (or may be) subject to permit review requirements.
3. "MODIFICATION of a SOURCE" means that (1) you already have emission units at your facility, (2) you are making physical or operational changes to the facility, (3) those proposed changes could result in a net emission increase of a regulated pollutant (or the emission of a regulated pollutant not presently being emitted), and (4) that physical or operational change is (or may be) subject to permit review requirements.
4. “RELOCATION of a SOURCE” means that you are relocating emission units from a facility in one location to a new or existing facility in another location and that relocation is (or may be) subject to permit review.
5. “PERMIT AMENDMENT” means that you have an effective air permit for your source, and you need changes made to that permit that do not qualify as a “MODIFICATION of a SOURCE”.
6. "OTHER (SPECIFY)" means you intend to make a change to your facility, you do not know what air permitting requirements apply, and you wish for DEQ to evaluate the change for you and determine which requirements apply. Fill out the Form 7 as completely as possible and describe in a letter what you wish to do.

The listed regulations detail the various types of air pollution permits. Please indicate which of these you **believe** are applicable to this application. (More than one may apply). Sections of the regulations may be downloaded from the DEQ web site at <https://www.deq.virginia.gov/laws-regulations/air>

**EXPLANATION OF PERMIT REQUEST –** Provide a brief narrative explanation or description of the permit request, including but not limited to, new units being added/modified, change in throughputs, changes to permit conditions, what type of facility it is, etc.

**IS THE FACILITY DESIGNED TO BE PORTABLE?** **–** [9VAC5-80-1110 B](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1110/) defines "portable", to mean an emissions unit that is designed to have the capability of being moved from one location to another for the purpose of operating at multiple locations and storage when idle Indications of portability include, but are not limited to, wheels, skids, carrying handles, dolly, trailer, or platform. If this facility is already permitted as a portable facility, list the date of the effective permit.

**IS THIS AN APPLICATION TO BE PERMITTED AS A PORTABLE PLANT?** **–** If the facility is designed to be portable, indicate whether or not you wish to have the permit contain specific conditions that will acknowledge this fact, so that the facility may be relocated without a new permit in accordance with [9VAC5-80-1105 A.1.c](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1105/).

**IS THIS A NOTIFICATION OF RELOCATION OF A PORTABLE FACILITY? –** [9VAC5-80-1105 A.1.c](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1105/) allows the relocation of a properly permitted portable facility to be exempt from permitting requirements, as long as it meets certain requirements, one of which is timely notification of the relocation. This notification should be sent to the Director of the DEQ Regional Office into whose area of responsibility the facility will be relocated. The 15-day notification period begins when DEQ receives the notification. Submission of pages 10 through 12 of this Form 7 may be used for that notification (with “RELOCATION of a SOURCE” marked on Page 11). However, use of this form for that purpose is not required. Note that a site map and documentation of site suitability should accompany this form or whatever means of notification is used. Include the registration number of any stationary source that will be co-located with the portable facility at the new site.

Site suitability may be documented by the use of a properly certified Local Governing Body Certification Form from the locality to which the facility will be relocated, although that form is not required for this purpose. Contact the appropriate DEQ Regional Office for instructions. DEQ will make a determination of site suitability based upon regional and local requirements.

**PRODUCTS MANUFACTURED/SERVICED** **–** Indicate the type of business in which this facility is engaged, listing products produced and/or services performed.

**SIC CODE(S)** **–** Provide all 4‑digit Standard Industrial Classification Code(s) for this facility and for the process(es). Place primary SIC in the first set of blocks.

Reference website: <https://www.osha.gov/data/sic-search>

**NAICS CODE(S)** **–** Provide all 6‑digit North American Industry Classification System Code(s) for this facility and for the process(es). Place primary NAICS in the first set of blocks.

Reference website: <https://www.census.gov/naics/>

**FACILITIES UNDER COMMON OWNERSHIP** **–** List the facilities in Virginia that are owned by the applicant company, its subsidiaries, and its parent company. Include air permit registration number of facility if known.

**MILESTONE DATES** **–** List all dates pertinent to this application as accurately as possible. For start-up dates, provide each relevant date as it might affect emissions, e.g., start-up of each unit, modification of each unit, imposition of or changes in permitted emissions for each unit.

1. **Page 13 – Fuel Burning Equipment**

**UNIT REF. NO. –** Assign a unique reference number for each piece of fuel burning equipment. If the facility has other equipment already registered, do not repeat those reference numbers. **NOTE:** Where a unit burns more than one fuel, assign a separate line for each, pegged to the unit (e.g., #1A for oil, #1B for the same unit burning coal, etc.).

**EQUIPMENT MANUFACTURER, TYPE AND MODEL NO.** **–**Provide the nameplate information for each piece of equipment.

**DATE OF MANUF. –** Give the date that each emission unit was (or will be) manufactured.

**DATE OF CONST. –** Give the date that each emission unit was (or will be) constructed in place.

**MAXIMUM RATED INPUT HEAT CAPACITY FOR EACH FUEL** **–** Provide the manufacturer's maximum rated heat input in units of Million Btus per hour based on the nameplate rating or maximum fuel usage.

**TYPE OF FUEL** – Identify all the types of fuel that will be burned by each referenced piece of equipment and the corresponding data for each fuel type. If used in a process, relate this to the appropriate process.

**TYPE OF EQUIPMENT** **–** Use Code A at the bottom of the page.

**USAGE** **–** Use Code B at the bottom of the page.

**REQUESTED THROUGHPUT –** Provide the requested throughput of the emission unit in units of hours of operation per year OR fuel per year (e.g., gallons per year, cubic feet per year, etc.) Specify which option is chosen and only one option can be chosen. These numbers may be used to establish air permit limits and should be consistent with calculated emissions.

**FEDERAL REGULATIONS THAT APPLY** – List all the federal regulations ([New Source Performance Standards (NSPS) in 40 CFR Part 60](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr60_main_02.tpl), [Maximum Achievable Control Technologies (MACT) in 40 CFR Part 63](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr63_main_02.tpl), etc.) that apply to the emission unit.

1. **Page 14 – Stationary Internal Combustion Engines**

**UNIT REF. NO. –** Assign a unique reference number for each stationary internal combustion engine. If the facility has other equipment already registered, do not repeat those reference numbers. **NOTE:** Where a unit burns more than one fuel, assign a separate line for each, pegged to the unit (e.g., #1A for oil, #1B for the same unit burning bio-diesel, etc.).

**EQUIPMENT MANUFACTURER, TYPE AND MODEL NO.** **–** Provide the nameplate information for each piece of equipment.

**DATE OF MANUF. –** Give the date that each emission unit was (or will be) manufactured.

**DATE OF CONST. –** Give the date that each emission unit was (or will be) constructed in place.

**OUTPUT BRAKE HORSEPOWER** **–** Provide the manufacturer's maximum rated output capacity in units of brake horsepower (also known as mechanical horsepower).

**OUTPUT ELECTRICAL POWER –** Provide the manufacturer's maximum rated output electrical power in units of kilowatts.

**TYPE OF FUEL** – Identify all the types of fuel that will be burned by each referenced piece of equipment and the corresponding data for each fuel type. If used in a process, relate this to the appropriate process.

**USAGE** **–** Use Code C at the bottom of the page.

**REQUESTED THROUGHPUT –** Provide the requested throughput of the emission unit in units of hours of operation per year **OR** fuel per year (e.g., gallons per year, cubic feet per year, etc.) Specify which option is chosen and only one option can be chosen. These numbers may be used to establish air permit limits and should be consistent with calculated emissions.

**FEDERAL REGULATIONS THAT APPLY** – List all the federal regulations ([New Source Performance Standards (NSPS) in 40 CFR Part 60](http://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr60_main_02.tpl), [Maximum Achievable Control Technologies (MACT) in 40 CFR Part 63](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr63_main_02.tpl), etc.) that apply to the emission unit.

1. **Page 15 – Liquid and/or Solid Waste Incinerators**

**UNIT REF. NO. –** Assign a unique reference number for each incinerator. If the facility has other equipment already registered, do not repeat those reference numbers. **NOTE:** Where a unit incinerates more than one waste type, assign a separate line for each, pegged to the unit.

**EQUIPMENT MANUFACTURER, TYPE AND MODEL NO.** **–** Provide the emission unit manufacturer and model number. Include a diagram of the unit and specify any special features. If the unit is used for energy recovery, provide this information on the Fuel Burning Equipment page.

**DATE OF MANUF. –** Give the date that each emission unit was (or will be) manufactured.

**DATE OF CONST. –** Give the date that each emission unit was (or will be) constructed in place.

**INCINERATOR MAXIMUM RATED CAPACITY** – Provide the maximum design input capacity in units of pounds per hour of waste type disposed of in this emission unit.

**BURNER RATED CAPACITY** – Provide the maximum rated heat input of the primary and secondary chamber burners in units of Btus per hour.

**MINIMUM CHAMBER TEMPERATURE –** Indicate the minimum temperatures which the burners in the primary and secondary chambers are designed to maintain while incinerating waste in units of degrees Fahrenheit.

**REQUESTED THROUGHPUT TO BE INCINERATED** – Provide the requested throughput amount of waste material expected to be incinerated in a 1-hour period and on an annual basis. For an air permit limit on this incinerator, this amount would be a reasonable and comfortable limit, taking future growth into account. These numbers may be used to establish air permit limits and should be consistent with calculated emissions.

**INCINERATOR TYPE** **–** Use Code D at the bottom of the page.

**WASTE TYPE** – Use Code E at the bottom of the page.

**MINIMUM SECONDARY CHAMBER RETENTION TIME** – Provide the minimum flue gas retention time in the secondary chamber at the specified minimum temperature in units of seconds.

**BURN DOWN CYCLE TIME** – Provide the minimum burn-down time recommended by the manufacturer or the time required to consume all combustible material, whichever is greater, in units of hours.

**FEDERAL REGULATIONS THAT APPLY** – List all the federal regulations ([New Source Performance Standards (NSPS) in 40 CFR Part 60](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr60_main_02.tpl), [Maximum Achievable Control Technologies (MACT) in 40 CFR Part 63](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr63_main_02.tpl), etc.) that apply to the emission unit.

1. **Page 16 – Processing, Manufacturing, Surface Coating and Degreasing Operations**

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**PROCESS OR OPERATION NAME** **–** Label each emission unit with the applicable process or operation, starting with the initial step in the manufacturing process, followed by succeeding logical manufacturing steps until the process is complete.

**EQUIPMENT MANUFACTURER, TYPE, AND MODEL NO.** **–** Provide the nameplate information for each piece of equipment.

**DATE OF MANUF. –** Give the date that each emission unit was (or will be) manufactured.

**DATE OF CONST. –** Give the date that each emission unit was (or will be) constructed in place.

**MAXIMUM RATED CAPACITY** – Provide the maximum rated input capacity of the process or operation in units of measure per hour.

**REQUESTED THROUGHPUT –** Provide the requested throughput of feed material expected to be processed (hourly, daily, and yearly) and/or output as needed. Specify units. These numbers may be used to establish air permit limits and should be consistent with calculated emissions.

**FEDERAL REGULATIONS THAT APPLY** – List all the federal regulations ([New Source Performance Standards (NSPS) in 40 CFR Part 60](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr60_main_02.tpl), [Maximum Achievable Control Technologies (MACT) in 40 CFR Part 63](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr63_main_02.tpl), etc.) that apply to the emission unit.

1. **Page 17 – Inks, Coatings, Stains, and Adhesives**

This page is intended to address volatile organic compounds (VOCs) and hazardous air pollutants (HAPs) resulting from application of inks, coatings, or stains. Each page may describe these pollutants from a single emissions unit.

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**COATING MATERIAL** **–** List typical coatings and a design, worst case coating type, e.g., topcoat having the highest percentage of VOCs and highest of each toxic component content as applied to the substrate.

**NOTE: Where the term "coating" is used in these instructions, the instructions may also refer to inks, stains, or adhesives**.

**COATING USE** **–** Choose the coating usage type from the Code F list at the bottom of the page, and list the letter or letter and number combination that describes the coating use. Use more than one if that individual coating formulation has multiple uses. If "Other Coating" is selected, describe.

**LBS. VOC IN COATING AS APPLIED** **–** List the VOC content of the coating as it is applied to the substrate including any added solvent, in units of (1) Pounds (lbs.) VOC per gallon of coating, (2) lbs. VOC per gallon coating, minus water and exempt solvents (compounds that are exempted from the definition of VOCs as defined in [9VAC5-10-20](https://law.lis.virginia.gov/admincode/title9/agency5/chapter10/section20/)), and (3) lbs. VOC per gallon coating solids. The above information should be calculated based on coating and solvent Environmental Data Sheets, Material Safety Data Sheets (MSDS), or Certified Product Data Sheets (CPDS) available from the coating supplier or manufacturer. Show calculations, if appropriate. If you have questions, please contact the Regional Office.

**VOC CONTROL METHOD –** Choose the appropriate number and/or letter code from the Code G list. If "Other" is selected, please describe.

**SOLIDS TRANSFER EFFICIENCY** **–** List the transfer efficiency as the ratio of the amount of coating solids deposited on the product to the amount of solids in the coating as applied.

**COATING DENSITY AS APPLIED** **–** List the density of the coating as applied to the substrate in units of pounds per gallon (lbs/gal). Show calculations if coating is thinned or reduced.

**MAXIMUM COATING USAGE AS APPLIED** **–** List the maximum expected usage of the individual coating or coating type in terms of gallons per hour (gal/hr) and gallons per year (gal/yr).

**HAZARDOUS AIR POLLUTANTS (HAPS) –** List the individual HAP components of the coating on the lines. For each hazardous air pollutant, give the name and Chemical Abstract Services (CAS) Number.

**LBS. HAP PER GALLON OF COATING AS APPLIED** **–** For each HAP component, list the pounds (lbs) of HAPs per gallon of coating as applied to the substrate. Attach sample calculations, including any emission factors used, and MSDS or CPDS sheets, if appropriate.

1. **Pages 18 and 19 – VOC/Petroleum Liquid Storage Tanks**

To estimate air emissions from tanks, please download the [TANKS Emissions Estimation Program Software.](https://www3.epa.gov/ttnchie1/software/tanks/)

For questions on the TANKS Software: [TANKS Software Frequent Questions](https://www3.epa.gov/ttn/chief/faq/tanksfaq.html)

**Page 18:**

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**TANK TYPE –** Use Code H at the bottom of the page.

**SOURCE OF TANK CONTENTS** – Use Code I at the bottom of the page.

**DATE OF MANUF.** –Give the date that each emission unit was (or will be) manufactured.

**DATE OF CONST. –** Give the date that each emission unit was (or will be) constructed in place.

**MATERIAL STORED** **–** List all possible contents for each tank for mixtures; include maximum percent by weight of each component on a separate line.

**MAXIMUM TRUE VAPOR PRESSURE** **–** Include the maximum true vapor pressure of each component at storage conditions in terms of absolute pressure for mixtures (see definition of True Vapor Pressure in [9VAC5-10-20](https://law.lis.virginia.gov/admincode/title9/agency5/chapter10/section20/)).

**DENSITY** **–** List the density of the stored material. For mixtures, give the density of each component.

**MAXIMUM AVERAGE STORAGE TEMPERATURE** **–** List the maximum average temperature at which the material is stored in units of Fahrenheit.

**TANK DIAMETER** – List the tank diameter in units of feet.

**TANK CAPACITY** **–** List the tank capacity in units of gallons.

**REQUESTED THROUGHPUT –** Provide the requested throughput of the emission unit in units of gallons per year (gal/yr). These numbers may be used to establish air permit limits and should be consistent with calculated emissions.

**FEDERAL REGULATIONS THAT APPLY** – List all the federal regulations ([New Source Performance Standards (NSPS) in 40 CFR Part 60](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr60_main_02.tpl), [Maximum Achievable Control Technologies (MACT) in 40 CFR Part 63](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr63_main_02.tpl), etc.) that apply to the emission unit.

**Page 19:**

**TANK COLOR ‑ SHELL/ROOF** **–** List the color(s) of shell and roof of the tank.

**For Fixed Roof Tanks:**

**INTERNAL TANK HEIGHT OR LENGTH** **–** For a vertical tank, list the height in units of feet. For a horizontal tank, list the length in units of feet.

**MAXIMUM HOURLY FILLING** **–** Maximum gallons that could be pumped into the tank in one hour, starting with an empty tank.

**TYPE OF ROOF** **–** For external fixed roof tanks, list the type of roof (cone or dome).

**CONE HEIGHT AND SLOPE** **–** For external fixed roof tanks with a cone roof, list the height in units of feet and the slope in units of feet per feet.

**DOME HEIGHT AND RADIUS** **–** For external fixed roof tanks with a dome roof, list the height in units of feet and the radius in units of feet.

**For Floating Roof Tanks:**

**SEAL TYPE** **–** Use Code J at the bottom of the page.

**MAXIMUM HOURLY WITHDRAWAL** **–** Maximum gallons that could be withdrawn from the tank in one hour, starting with a full tank.

**SELF SUPPORTING** **–** For internal floating roof tanks, identify if the tank if self-supporting (yes or no).

**NO. OF COLUMNS** – For internal floating roof tanks, if the tank is NOT self-supporting, list the number of columns.

**COLUMN DIAMETER** **–** For internal floating roof tanks, if the tank is NOT self-supporting, list the column diameter in units of feet.

**\*\*Note:** If the TANKS program is used for emission calculations, please note that the TANKS program has not been updated with roof landing losses calculations for internal floating roof tanks. However, it is possible to estimate roof landing losses in TANKS by using a portion of the guidance developed for degassing and cleaning a tank by modeling the vapor space under the roof as a fixed roof tank and calculating the emissions from one turnover. This is less accurate than using [Section 7.1.3.2.2 of AP-42](https://www.epa.gov/ttn/chief/ap42/ch07/index.html).

1. **Page 20 – Loading Racks and Oil-Water Separators**

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**NAME OF PRODUCT LOADED OR RECOVERED** **–**For loading racks, list all possible materials loaded for each rack. For oil‑water separators, list all possible materials recovered.

**MAXIMUM HOURLY THROUGHPUT** **–** Provide the expected maximum gallons to be loaded from the rack or entering the oil‑water separator in one hour.

**REQUESTED ANNUAL THROUGHPUT –** Provide therequested annual throughput in units of gallons to be loaded from the rack or entering the oil‑water separator in one year. This amount would be a reasonable and comfortable limit considering future growth. These numbers may be used to establish air permit limits and should be consistent with calculated emissions.

**FEDERAL REGULATIONS THAT APPLY** **–** List all the federal regulations ([New Source Performance Standards (NSPS) in 40 CFR Part 60](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr60_main_02.tpl), [Maximum Achievable Control Technologies (MACT) in 40 CFR Part 63](https://www.ecfr.gov/cgi-bin/text-idx?tpl=/ecfrbrowse/Title40/40cfr63_main_02.tpl), etc.) that apply to the emission unit.

**For Loading Racks Only:**

**TYPE OF LOADING** **–** Use Code K at the bottom of the page.

**HATCH VAPOR CLOSURE ON LOADING ARMS** **–** Use Code L at the bottom of the page.

**For Oil-Water Separators Only**

**TYPE OF ENCLOSURE** **–** Use Code M at the bottom of the page.

1. **Page 21 – Fumigation Operations**

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**OBJECT OR PRODUCT TO BE FUMIGATED** **–** Provide each type of product or object to be fumigated. For example: lumber, tobacco, silo, pallets, mattresses, etc. If the facility will be fumigating many different types of commodities, then the commodities may be grouped. For example: food products, wood products, etc.

**CONTAINMENT SYSTEM –** Provide the type of containment system to be used during fumigation. For example: Sealed silo, Sealed Containers, Tarp, Sealed warehouse, etc.

**FUMIGANT –** Provide type of fumigant to be used. For example: methyl bromide or phosphine

**MAXIMUM DAILY FUMIGANT USAGE** **–** Provide the maximum expected amount of fumigant to be used in one calendar day. If multiple fumigations will occur during the same day, these should be added together to obtain the daily usage. If more than one type of fumigant is to be used, maximum daily amounts should be provided for each fumigant. Units should be provided in pounds (methyl bromide) or grams (phosphine) per day.

**MAXIMUM ANNUAL FUMIGANT USAGE** **–** Provide the maximum annual amount of fumigant to be used in a year. If more than one type of fumigant is to be used, maximum annual amounts should be provided for each fumigant. Units should be provided in pounds or tons (methyl bromide) or grams (phosphine) per year.

**ESTIMATED NUMBER OF FUMIGANT EVENTS PER YEAR** – Multiple units fumigated at the same time in the same area can be considered one fumigation event.

**AERATION METHOD** **–** Indicate whether aeration will occur naturally or using fans or other mechanical methods.

**DISTANCE FROM FUMIGATION OPERATION TO PROPERTY OR FENCELINE** **–** Provide the distance from the fumigation operation to the property or fence line. If the property is not fenced, please note this on the form.

1. **Page 22 – Air Pollution Control and Monitoring Equipment**

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**VENT/STACK NO.** **–** Assign a unique vent/stack number for each vent or stack through which the process or equipment identified by this reference number exhausts.

**DEVICE REF. NO. –** Assign a unique pollution control device reference number(s).

**POLLUTANT/PARAMETER** – List all the pollutants emitted from this process/equipment that are controlled and/or monitored. List all surrogate parameters of the process/equipment that are monitored (e.g. ‑ opacity, CO2, etc.).

**Air Pollution Control Equipment:**

**MANUFACTURER AND MODEL** **–** List the manufacturer and model of the control equipment associated with the pollutant listed in the preceding column.

**TYPE** **–** Use Code N at the bottom of the page.

**PERCENT EFFICIENCY** **–** List the percent control efficiency for the control equipment and associated pollutant.

**Monitoring Instrumentation:**

**SPECIFY TYPE, MEASURED POLLUTANT, AND RECORDER USED** **–** Please list:

* Type: The manufacturer and model number of the stack gas monitor used to measure emissions of the measured pollutant. List opacity monitors in association with particulate/PM10/PM2.5 emissions.
* Measured Pollutant: The pollutant that is measured by the monitoring equipment.
* Recorder Used: The type of recorder associated with the monitor (e.g., strip chart, data logger, etc.).

1. **Page 23 – Air Pollution Control Equipment – Supplemental Information**

**DEVICE REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**TYPE** **–** Use Code N at the bottom of the page.

**NOTE: For the remaining columns, the applicable control device type numbers (see Code N) for which this information is required are listed in parentheses on the form.**

**LIQUID FLOW RATE** **–** List in units of gallons per minute (gpm).

**LIQUID MEDIUM** **–** Specify the type of liquid used in the control equipment, and the pH. For condensers, specify inlet temperatures of condensing medium (water, glycol, etc.) and inlet temperature of gas stream.

**CLEANING METHOD** **–** Specify the method of cleaning the control equipment (e.g., a baghouse, No. 9a).

**NUMBER OF FIELDS or SECTIONS** **–** List the number of fields or chambers for ESPs (No. 10), or number of chambers for baghouses (No. 9).

**AIR-TO-CLOTH RATIO** **–** List in units of feet per minute (fpm) or as specified by manufacturer (cubic feet per minute gas flow to square feet of cloth).

**FILTER MATERIAL** **–** List the type of material used for the baghouse filters.

**INLET TEMP.** **–** List the temperature at the inlet of the control equipment in units of degrees Fahrenheit.

**REGENERATION METHOD & CYCLE TIME** **–** List the regeneration method (steam stripping, hot air, etc.) and cycle time in units of seconds for adsorbers (No. 19). If regeneration is done offsite, please state so.

**CHAMBER TEMP.** **–** List the combustion temperature of afterburner chamber in units of degrees Fahrenheit.

**RETENTION TIME** **–** List the retention time for the control equipment in units of seconds.

**PRESSURE DROP** **–** List the pressure drop across the control equipment in units of inches of water.

1. **Page 24 – Stack Parameters and Fuel Data**

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**VENT/STACK NO.** **–** Assign a unique vent/stack number for each vent or stack through which the process or equipment identified by this reference number exhausts.

**Vent/Stack or Exhaust Data**:

**VENT/STACK CONFIGURATION** **–** Use Code O at the bottom of the page.

**VENT/STACK HEIGHT** **–** List the exit height from the ground level in units of feet.

**EXIT DIAMETER** **–** List the inside diameter of the vent/stack at its exit in units of feet. For rectangular vents, provide length and width of the vent/stack at its exit in units of feet.

**EXIT GAS VELOCITY** **–** List the velocity in units of feet per second of the stack gas as it exits the vent/stack.

**EXIT GAS FLOW RATE** **–** List the volume of the flow in units of actual cubic feet per minute.

**EXIT GAS TEMPERATURE** **–** List the exit gas temperature in units of degrees Fahrenheit.

**Fuel(s) Data:**

**TYPE OF FUEL** **–** Identify all the types of fuel that will be burned by each referenced piece of equipment and the corresponding data for each fuel type.

**HIGHER HEATING VALUE** **–** Provide the higher heating value of the specified fuel in units of Btus per unit of fuel.

**MAXIMUM RATED BURNED/HR -** Provide the maximum rated fuel input at maximum design capacity in units such as pounds, gallons, or cubic feet per hour.

**MAXIMUM PERCENT SULFUR** ‑ Identify the highest percent sulfur content for the fuel.

**MAXIMUM PERCENT ASH** ‑ Identify the highest percent ash content for the fuel.

1. **Page 25 – Proposed Permit Limits for Criteria Pollutants**

**UNIT REF. NO. ‑** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**PROPOSED PERMIT LIMITS FOR CRITERIA POLLUTANTS** - List the emission rates to the atmosphere for the pollutants indicated in pounds per hour and tons per year. Provide detailed calculations including assumed control efficiency of control equipment (if applicable) and using the proposed limits on material, throughput and/or hours of operation per year.

**CRITERIA POLLUTANTS** are defined as follows:

* Particulate Matter (PM) – Any airborne finely divided solid material with an aerodynamic diameter smaller than 100 micrometers.
* Particulate (PM10) - Particulate matter with an aerodynamic diameter less than or equal to 10 micrometers (includes filterable and condensable).
* Particulate (PM2.5) - Particulate matter with an aerodynamic diameter less than or equal to 2.5 micrometers (includes filterable and condensable).
* Sulfur Oxides (SOX) - Measured as sulfur dioxide (SO2).
* Nitrogen Oxides (NOX) - All oxides of nitrogen except nitrous oxide.
* Carbon Monoxide (CO) - Colorless, odorless, tasteless gas.
* Lead (Pb) – Metal.
* Volatile Organic Compounds (VOCs) - (See definition in [9VAC5-10-20](https://law.lis.virginia.gov/admincode/title9/agency5/chapter10/section20/)). Do not include perchloroethylene as a VOC; list it as a hazardous air pollutant (HAP) on page 26 of the Form 7 Application. The following common compounds are currently exempt from the definition of VOC (however, items 4 and 5 below are still to be reported as toxic pollutants on page 26):

1. Acetone
2. Methane
3. Ethane
4. 1,1,1-trichloroethane (methyl chloroform)
5. Methylene chloride
6. Trichlorofluoromethane (CFC-11)
7. Dichlorodifluoromethane (CFC-12)
8. Chlorodifluoromethane (HCFC-22)
9. Trifluoromethane (HFC-23)
10. 1,1,2-trichlorotrifluoroethane (CFC-113)
11. 1,2-dichlorotetrafluoroethane (CFC-114)
12. Chloropentafluoroethane (CFC-115)
13. Dichlorotrifluoroethane (HCFC-123)
14. Tetrafluoroethane (HFC-134a)
15. Dichlorofluoroethane (HCFC-141b)
16. Chlorodifluoroethane (HCFC-142b)
17. **Page 27 – Proposed Permit Limits for Toxic Pollutants/HAPs**

Complete this page for any new emissions or increased emissions of toxic pollutants or HAPs resulting from the Proposed Facility (from a new plant, or from any new, modified, reconstructed, or debottlenecked processes or equipment at an existing plant. It is not necessary to list each toxic or HAP emitted from the source unless so directed by the [DEQ Regional Office](https://www.deq.virginia.gov/get-involved/about-us/contact-us). Then, for each toxic pollutant listed, which is not exempt by [9VAC5-60-300 C.3, 4 or 5, or D, E, or F](https://law.lis.virginia.gov/admincode/title9/agency5/chapter60/section300/) or [9VAC5-80-1105 F](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1105/) of the Regulations, list the total source-wide emissions of that pollutant. Compliance is based on total toxic emissions from the source.

**UNIT REF. NO. ‑** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**PROPOSED PERMIT LIMITS FOR TOXIC POLLUTANTS/HAPS** - List the emission rates to the atmosphere for the pollutants indicated in pounds per hour and tons per year. Provide detailed calculations including assumed control efficiency of control equipment (if applicable) and the proposed limits on material, throughput and/or hours of operation per year.

**CAS NO.** - List the Chemical Abstract Services (CAS) number for each listed pollutant.

1. **Page 26 – Proposed Permit Limits for Other Regulated Pollutants**

**UNIT REF. NO. ‑** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**PROPOSED PERMIT LIMITS FOR OTHER REGULATED POLLUTANTS** - List the emission rates to the atmosphere for all pollutants listed in the definition of “regulated pollutants” in Article 6 ([9VAC5-80-1110 C](https://law.lis.virginia.gov/admincode/title9/agency5/chapter80/section1110/)) of the Regulations except for the Criteria Pollutants (PM, PM10, PM2.5, SO2, NOX, CO, VOC and Pb) and the toxic/HAP pollutants listed on the toxic/HAP pollutant listing in the front of this Instructions document. These pollutants include: Fluorides, Sulfuric Acid Mist, Hydrogen Sulfide (H2S), Total Reduced Sulfur (including H2S), Reduced Sulfur Compounds (including H2S), Municipal Waste Combustor Organics (measured as total tetra-through octa-chlorinated dibenzo-p-dioxins and dibenzofurans), Municipal Waste Combustor Metals (measured as particulate matter), Municipal Waste Combustor Acid Gases (measured as the sum of SO2 and HCl), and Municipal Solid Waste Landfill Emissions (measured as nonmethane organic compounds). Provide detailed calculations of the emission rates, using (for the proposed controlled emission rates) the proposed control efficiency of control equipment, and using the proposed limits on material, throughput and/or hours of operation per year.

1. **Page 28 – Proposed Permit Limits for Greenhouse Gases (GHGs) on Mass Basis**

**IMPORTANT NOTICE: THIS PAGE IS FOR PSD MAJOR SOURCES ONLY!**

Please see [9VAC5 Chapter 85](https://law.lis.virginia.gov/admincode/title9/agency5/chapter85/#C0085) for more information on Greenhouse Gases.

**UNIT REF. NO. ‑** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**PROPOSED PERMIT LIMITS FOR GHGs POLLUTANTS ON MASS BASIS** - List the proposed permit emission limits for the GHGs pollutants in pounds per hour and tons per year. Provide detailed calculations including assumed control efficiency of control equipment (if applicable) and using the proposed limits on material, throughput and/or hours of operation per year.

1. **Page 29 – Proposed Permit Limits for Greenhouse Gases (GHGs) on CO2 Equivalent Emissions (CO2e) Basis**

**IMPORTANT NOTICE: THIS PAGE IS FOR PSD MAJOR SOURCES ONLY!**

Please see [9VAC5 Chapter 85](https://law.lis.virginia.gov/admincode/title9/agency5/chapter85/#C0085) for more information on Greenhouse Gases.

**UNIT REF. NO. ‑** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**PROPOSED PERMIT LIMITS FOR GHGs POLLUTANTS ON CO2 EQUIVALENT BASIS** - List the proposed permit emission limits for the GHGs pollutants on a CO2e basis in pounds per hour and tons per year. Provide detailed calculations including assumed control efficiency of control equipment (if applicable) and using the proposed limits on material, throughput and/or hours of operation per year.

**\*\*Note:** The [information on converting mass based emissions to CO2e based emissions](#MassBasedEmissionsToCO2e) is provided in the instructions for *Page 32 of Form 7 - Baseline Actual Emissions (BAE) For Greenhouse Gases (GHGs) Pollutant Emissions on CO2 Equivalent Emissions (CO2e) Basis (page 31 of this document*.)

1. **Page 30 – Baseline Actual Emissions (BAE) for Criteria Pollutants**

**IMPORTANT NOTICE: THIS PAGE IS FOR PSD OR MAJOR NONATTAINMENT SOURCES ONLY!**

**UNIT REF. NO. ‑** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**CRITERIA POLLUTANTS** are defined as follows:

* Particulate Matter (PM) – Any airborne finely divided solid material with an aerodynamic diameter smaller than 100 micrometers.
* Particulate (PM10) - Particulate matter with an aerodynamic diameter less than or equal to 10 micrometers (includes filterable and condensable).
* Particulate (PM2.5) - Particulate matter with an aerodynamic diameter less than or equal to 2.5 micrometers (includes filterable and condensable).
* Sulfur Oxides (SOX) - Measured as sulfur dioxide (SO2).
* Nitrogen Oxides (NOX) - All oxides of nitrogen except nitrous oxide.
* Carbon Monoxide (CO) - Colorless, odorless, tasteless gas.
* Lead (Pb) – Metal.
* Volatile Organic Compounds (VOCs) - (See definition in [9VAC5-10-20](https://law.lis.virginia.gov/admincode/title9/agency5/chapter10/section20/)). Do not include perchloroethylene as a VOC; list it as a hazardous air pollutant (HAP) on page 26 of the Form 7 Application. The following common compounds are currently exempt from the definition of VOC (however, items 4 and 5 below are still to be reported as toxic pollutants page 26):

1. Acetone
2. Methane
3. Ethane
4. **1,1,1-trichloroethane (methyl chloroform)**
5. **Methylene chloride**
6. Trichlorofluoromethane (CFC-11)
7. Dichlorodifluoromethane (CFC-12)
8. Chlorodifluoromethane (HCFC-22)
9. Trifluoromethane (HFC-23)
10. 1,1,2-trichlorotrifluoroethane (CFC-113)
11. 1,2-dichlorotetrafluoroethane (CFC-114)
12. Chloropentafluoroethane (CFC-115)
13. Dichlorotrifluoroethane (HCFC-123)
14. Tetrafluoroethane (HFC-134a)
15. Dichlorofluoroethane (HCFC-141b)
16. Chlorodifluoroethane (HCFC-142b)

**AVERAGE ACTUAL ANNUAL EMISSIONS TO THE ATMOSPHERE OF CRITERIA POLLUTANTS -** The method of calculating BAE varies for Electric Utility Steam Generating Units (EUSGU) and for all other types of emissions units (non-EUSGU).

BAE for an existing EUSGU: BAE for an existing EUSGU is defined as the average actual emissions (in tpy) calculated over a consecutive 24-month period of actual operation, within the 5-year period immediately preceding when the owner *begins actual construction* on the project. A 24-month period outside of the aforementioned 5-year period may be used upon a determination by the DEQ Regional Office that it is more representative of normal source operation (please provide documentation to support such claim).

The criteria for determining BAE for an existing EUSGU, is as follows:

* Include all fugitive emissions to the extent quantifiable and all emissions associated with start-up, shutdown and malfunction.
* Adjust the calculated average emission rate to account for non-compliant emissions. Adjust it downward for periods during the 24-months when actual emissions exceeded an emission limitation that applied during the 24-month period. The actual emissions used in the calculation may not exceed enforceable emission limits.
* When a project involves multiple emissions units, only one consecutive 24-month period should be used for all affected units (including debottlenecked units) in determining BAE for a regulated NSR pollutant. The same consecutive 24-month period should be used for each different regulated NSR pollutant unless the source can demonstrate to the satisfaction of the Regional Office that an alternative consecutive 24-month period for a different pollutant or pollutants is more appropriate due to extenuating circumstances. The source must provide documentation to support such claim.
* BAE may not be established using any consecutive 24-month period for which there is inadequate information to determine actual annual emissions in tpy and for adjusting this amount. If documentation is missing or incomplete for any part of the selected 24-month period, a different consecutive 24-month period must be selected.

BAE for an existing non-EUSGU: BAE for an existing non-EUSGU is defined as the average actual emissions (in tpy) calculated over a consecutive 24-month period of actual operation, within the 5-year period immediately preceding either the date the owner *begins actual construction* on the project or the date a complete application for the proposed project is received, whichever is earlier. A 24-month period outside of the aforementioned 5-year period may be used upon a determination by the DEQ Regional Office that it is more representative of normal source operation (please provide documentation to support such claim).

The criteria for determining BAE for an existing non-EUSGU, is as follows:

* Include all fugitive emissions to the extent quantifiable and all emissions associated with start-up, shutdown and malfunction.
* Adjust the calculated average emission rate to account for non-compliant emissions. Adjust it downward for periods during the 24-months when actual emissions exceeded an emission limitation that applied during the 24-month period. The actual emissions used in the calculation may not exceed enforceable emission limits.
* Adjust the calculated average emission rate downward to exclude emissions that would have exceeded an emission limitation with which the facility must currently comply.
* When a project involves multiple emissions units, only one consecutive 24-month period should be used for all affected units (including debottlenecked units) in determining BAE for a regulated NSR pollutant. The same consecutive 24-month period should be used for each different regulated NSR pollutant unless the source can demonstrate to the satisfaction of the DEQ Regional Office that an alternative consecutive 24-month period for a different pollutant or pollutants is more appropriate due to extenuating circumstances (please provide documentation to support such claim).
* BAE may not be established using any consecutive 24-month period for which there is inadequate information to determine actual annual emissions in tpy and for adjusting this amount. If documentation is missing or incomplete for any part of the selected 24-month period, a different consecutive 24-month period must be selected.

BAE for a new emissions unit: When a new unit (a unit that has existed for less than 2 years) is changed by a project, the *baseline actual emissions* rate is zero if it has not yet begun operation and is equal to the unit’s PTE once it has begun to operate.

1. **Page 31 – Baseline Actual Emissions (BAE) for Greenhouse Gases (GHGs) Pollutant Emissions on Mass Basis**

**IMPORTANT NOTICE: THIS PAGE IS FOR PSD MAJOR SOURCES ONLY!**

Please see [9VAC5 Chapter 85](https://law.lis.virginia.gov/admincode/title9/agency5/chapter85/#C0085) for more information on Greenhouse Gases.

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**AVERAGE ACTUAL ANNUAL EMISSIONS TO THE ATMOSPHERE OF GHGs –** The method of calculating BAE for GHGs is the same as that for criteria pollutant emissions.

1. **Page 32 – Baseline Actual Emissions (BAE) for Greenhouse Gases (GHGs) Pollutant Emissions on CO2 Equivalent Emissions (CO2e) Basis**

**IMPORTANT NOTICE: THIS PAGE IS FOR PSD MAJOR SOURCES ONLY!**

Please see [9VAC5 Chapter 85](https://law.lis.virginia.gov/admincode/title9/agency5/chapter85/#C0085) for more information on Greenhouse Gases.

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**AVERAGE ACTUAL ANNUAL EMISSIONS TO THE ATMOSPHERE OF GHGs –** Convert the previously calculated BAE on mass basis to CO2e basis using GHG compounds associated global warming potential (GWP) published at [Table A-1 to Subpart A of 40 CFR Part 98.](https://www.ecfr.gov/cgi-bin/text-idx?SID=8b39fd325e59ccc735aee1c6490efdc3&mc=true&node=ap40.23.98_19.1&rgn=div9) The following example below illustrates this.

EXAMPLE:

BAE on mass basis for GHG compounds are following:

50,000 tons/yr (TPY) of CO2

60 TPY of Methane

1 TPY of Nitrous Oxide

5 TPY of HFC-32 (a hydrofluorocarbon)

3 TPY of PFC-14 (a perfluorocarbon)

Total BAE on mass basis = 50,000 + 60 + 1 + 5 + 3 = 50,069 TPY

The GWP *(see 40 CFR Part 98, Subpart A, Table A-1)* for each of the GHGs used in this example are:

|  |  |
| --- | --- |
| GHG | GWP |
| Carbon Dioxide | 1 |
| Nitrous Oxide | 310 |
| Methane | 21 |
| HFC-32 | 650 |
| PFC-14 | 6,500 |

BAE on CO2e basis for the GHG compounds are calculated below:

|  |  |
| --- | --- |
| Carbon Dioxide: | 50,000 TPY x 1 = 50,000 TPY CO2e |
| Nitrous Oxide: | 1 TPY x 310 = 310 TPY CO2e |
| Methane: | 60 TPY x 21 = 1,260 TPY CO2e |
| HFC-32: | 5 TPY x 650 = 3,250 TPY CO2e |
| PFC-14: | 3 TPY x 6,500 = 19,500 TPY CO2e |

Total BAE on CO2e basis = 50,000 + 310 + 1,260 + 3,250 + 19,500 = 74,320 TPY

1. **Page 33 – Operating Periods**

**UNIT REF. NO. –** Assign a unique reference number for each piece of equipment. If the facility has other equipment already registered, do not repeat those reference numbers.

**PERCENT ANNUAL USE/THROUGHPUT BY SEASON** **–** Give the percentage of time the process or equipment was operated (past five years), by the indicated seasons. Do the same for the proposed operation.

**NORMAL PROCESS/EQUIPMENT OPERATING SCHEDULE** **–** Indicate the normal operating schedule expected for the process equipment.

**MAXIMUM PROCESS/EQUIPMENT OPERATING SCHEDULE** **–** Indicate the maximum operating schedule expected for the process/equipment.

**MAXIMUM FACILITY OPERATING SCHEDULE** **–** Indicate the maximum number of hours of operation for the entire facility.